* Added numerical input box to USB Logging screen to change the log period (Modbus integer register 50)
* Switched the mapping for the IDEC logging screen, which now comes second, and the USB logging, which is now first