* Bug fix: Changing streams with MSVE buttons did not execute Mirror\_From\_Stream\_Table() vector
  + Changed logic to use long int (32bit) register instead of int (16bit), which fixed the problem
* Increased the number of serial comm. retries to avoid "host communication error" when saving configuration