* Data Logging screen now correctly recognizes FW v6.12 and below, skipping the USB Logging screen
  + Prevents users with v6.12.x and below from navigating to a screen which would cause the HMI to freeze (illegal Modbus register error)
* PID screens now display the text "minutes" next to the 'I' value
  + This is NOT an indication that the firmware is updated to a version that has the new PID, it's simply a new text box. (Firmware v6.12.6 and later use the new PID)
* Information screen now displays the subversion number (e.g. 6.12.**5**), if one exists
  + This change is cleverly backward compatible with previous firmware revisions that don't have a subversion
* Previous version: **3.14.2a** (ECO #300)
  + '14.2b' was never released, changes were rolled into '14.3a'
* Compatibility:
  + Compatible with all NEW screens (HG2G)
  + Compatible with all firmware dating back to at least 2013, and perhaps much older